Readme
------------------------

🔸 You only install the PrepperRadio firmware by the PrepperDock application.

➖ For Windows, start ‘PrepperDock-Win_v2025-xx-xx.exe’,
for Linux ‘PrepperDock-Linux-install_2025-xx-xx.run’.
➖ Follow the instructions in the ‘PrepperRadio Manual’ in chapter 2.3, available from the Home window of PrepperDock.

🔸 Quick instructions:
➖ Connect the radio with the appropriate cable.
➖ Start PrepperDock.
➖ Open the Q Connect window.
➖ Select the cable and Serial port.
➖ In Automagic Firmware, select ‘PrepperDock FW’.
➖ Put radio into update mode (hold down PTT button and turn radio on).
➖ PrepperDock will automatically load the firmware.
⚠️For the new K5 V3 and K1 models, for the first time, you must to must load a BandPlan (Config file), tick the “Write Calibration” box and click on “Write All”.

For everything else, read the manuals on the PrepperDock Home window.